{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"flags":["formulas_cached_only"]}
[{"$nulls":3},"Free household safety check list spreadsheet. "]
[]
[{"$nulls":5},"Safety Switches"]
[]
[]
[]
["ITEM ","Name"]
[]
[null,null,"6 MONTHLY"]
["safety switch 1","Lights"]
["safety switch 2","Lights"]
["safety switch 3","Power"]
["safety switch 4","Power"]
["safety switch 5","Power"]
["safety switch 6","Power"]
["safety switch 7","Cook top"]
["safety switch 8","Oven"]
["safety switch 9"]
["safety switch 10"]
[]
[]
[]
[]
["Notes","Check your state regulations for the recommended testing interval"]
[null,"Using the “test Button” is not a guarantee of correct operation only an indication that its working"]
[null,"Press the test button for 2 seconds if it does not trip at all call an electrician urgently."]
[null,"Safety switches are designed to trip in under 30 Ms or under 0.03 of a second."]
[null,"If you are renting a property ask for the safety switch test results."]
[null,"When purchasing a property have the the electrical installation tested including full results of the safety switches :"]
[null,"EG the Insulation test results in Meg Ohms "]
[null,"RCD 1   trip time in Ms at 30ma"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}